
== Created January 12, 2018 Emerson ATG 6500 Version 2.20 Release 1 ==

  New
	- Compatibility test with MS Windows 7 and Windows 10
	- Rebranding CSI to AMS
	- A 6410: Negative shifts are available again

  Bug fixes
	- Minor bug fixes




== Created November 8, 2016 Emerson CSI 6500 Version 2.15 Release 1 ==

  New
	- Seperation of A6910 into CSI 6500 Configuration and CSI 300 Configuration

  Bug fixes
	- Minor bug fixes
	- A6150 - Error in offline configuration fixed
	- A6125 - Error in configuration over A6824 fixed



== Created June 1, 2015 Emerson CSI Version 2.14 Release 1 ==

  New
	- A3910 Software relabeled to Emerson
	- A3910 Software integrated in setup package

  Bug fixes
	- Minor bug fixes

	
== Created December 4, 2014 Emerson CSI Version 2.13 Release 1 ==

  New
	- Transition values for A6210 Tandem Cone
	- Updated list of Converters

  Bug fixes
	- A6740 - Continuous function chart improvements
	- Sensor PR 9350 - Corrections for sensitivity parameter
	- Minor bug fixes

	
== Created November 4, 2013 Emerson CSI Version 2.12 Release 1 ==

  New
	- New output function in A6312 integrated

  Bug fixes
	- A6312, A6125

  
== Created July 5, 2013 Emerson CSI Version 2.11 Release 1 ==

  New
	- New monitor types A6150 and A6151 integrated

  Bug fixes
	- A6210, A6125, A6824

  
== Created March 20, 2013 Emerson CSI Version 2.10 Release 12 ==

  Bug fixes
	- Deviation #2792 : A6110 : The values for Danger alarm and Alert alarm are not displayed after the configuration has been received.
  
  
== Created January 17, 2013 Emerson CSI Version 2.10 Release 10 ==
  
  New
	- New monitor type 6210 Rod Drop integrated
  
== Created December 12, 2012 Emerson CSI Version 2.10 Release 01 ==
  
  Bug fixes
	- ABW 11-365 : A6125 : Check if the selected filter option is available on the module, otherwise an error message occurs.
	- ABW 11-376 : MMS3120 : The units of the selected operating mode are now the right ones. 
	- ABW 11-378 : Zoom in the online view of the analyze functions is now enabled
	- ABW 12-075 : A6630 : All settings are saved properly.
	- ABW 12-188 : A6630 : The property "Operating mode" can new be selected in the "channel clear" selection of the binary output.

	- If the amount of data in the data acquisition is expired, a warning message will now occur.
	
  Translations
	- Portuguese language added
	- Translations completed
	
  Miscellaneous
	- VxComm Drivers updated to Version 2.11.08
	- Dongle drivers updated
	- OPC Core Components updated


== Created June 17, 2011 Emerson CSI Version 2.08 Release 02 ==
  
  Bugfixes
  
  Translations



== Created May 19, 2011 Emerson CSI Version 2.08 Release 01 ==

  Windows 7 support

  New help files: now *.CHM files in the format of precompiled HTML format instead of *.HLP files
  (needed for Windows Vista and Windows 7) 

  Hungarian as additional language included
  
  Bugfix: now correct redraw of the GUI after a Windows logout / screenlock
  
  Integrated MMS6630 Temperature card (MMS6910 und MMS6855)
  
  Module internal negative version numbers will be marked as "Beta", but will be shown with positive version numbers 
  
  New version of password files, new logins for service + factory mode. All old accounts will be void!
  
  No more error message, if button "Cancel" is be pressed and the configuration is within wrong ranges
  
  Pre-Alarm of the module internal temperature may not be larger than the danger alarm any more.
  
  No more double mnemonics for menue entries

  New location of the password file   
  (C:\ProgramData\emerson\csi-6500-configuration\1.0, may vary between windows versions)
  
  Several smaller bugfixes





== Created February 05, 2010 Emerson CSI Version 2.07 Release 02 ==

MMS 6125:
  New parametrization dialog: Peak/Phase (Firmware version 156 and higher), new command "Measurement Peak Phase CH 1 + 2"
  
MMS 6312:
  Changes in parametrization dialog: "Number Measurements Average" to "Time Constant Acc.",
  Change: "Min. Rotational Speed" to "+- Acceleration" if Acceleration is selected,
  Correction of limits and units

MMS 631X:
  Automatical setting of new HW options, depending on subtype (6310/6312)

MMS 3410:
  Implementation of new config protocol, revision of parametrization dialogs





== Created on the 27.08.2009 Emerson CSI Version 2.07 Release 01 ==

Generally:
	In the dialog of the liniarisation the software control the values of wrong types. 
	If there is a comma in the entry of the sensor working area, you can not come out of this dialog.
	Error solved (MM)

	The virtual com driver has the new version 2.9.6. (Re-connect problems are solved)

	New help files for the programs MMS3910, MMS6910 und MMS6855.

MMS 6910:
	A new command for "Reset-Latch" is for the module MMS 6824 implemented.

MMS 6855:
	The OPC tags for the 3000 serial are new designed for English. The same is done for DOPS and DAPS.

	The module 331 is added.

	New channel description tags for all modules are implemented.

	If the dialog Service of the MMS 6350 Dops module opend, the software break down. 
	Error solved (MM)

MMS 6824:
	New sort register blocks are generated for values, alarms, Channel Clear aso.)
	
	A new command for reset latch is implemented.

MMS 6125:
	The parameter "integration frequency" could not send to the module. Allways the value 80 is send to the module.
	Error solved (MM)

MMS 6120:
	A new subtyp "MMS 6120 Smax" is added.



== Created on the 19.02.2009 Emerson CSI Version 2.06 Release 05 == 

Generally:
	In the Version 2.06 release 04 the setup shows wrong company logos. 
	Error solved (MM)
	
	The background colors of the main values are not change from green to red when the communication is lost.
	Error solved (MM)
	
	The default values of the current supply are changed for the sensor types 
	PR9268/20, PR9268/30, PR9268/200 und PR9268/300.


== Created on the 29.01.2009 Emerson CSI Version 2.06 Release 04 ==

Generally:
	We add the inVISU Dongle driver to the installation setup. 
	In the window dongle intsallation we add a new inVISU point.
	If this is choosed, the inVISU dongle driver will be installed at the end.
	
	We developed a new Subtype for the DAPS system. The programs MMS 6855 and MMS 6860 
	are increaced with this new type.
	
	The display of the MMS 631X could not show rotations over 10000 RPM with the unit behind. 
	Error solved (MM)

MMS 6910:
	In the configuration of the 631x was an error. If you give in rotations over 32767, 
	the next time you read out this values are changed in negative values.
	Error solved (MM)
	
	A compare function is added. It is possible to compare the PC configuration with a connected module 
	or with a stored file (*iMC6 oder *M6M) 

MMS 6855:
	We add new OPC Tag for the orda Na-Ne for the dynamic module types 6110, 6120, 6125 and 6140.

	Some program properties e.g. Global data directory are lost if the program stops at startup. 
	e.g. Dongle not found
	Error solved (MM)

	The OPC-Tags of the Module 6620 are sort new. It was importened to fit with the data collection.

	If you edit the root of the treeview, the program crach. 
	Error solved (MM)

	The qualitys of the OPC-Tags are set to bad after one communication error. This is now after 2 communication errors.

MMS 6740:
	By the module 6740 it was not possible to take one configuration from a module 
	and send it to an another module over the RS 232.
	Error solved (MM)

MMS 631X:
	A configuration file (*.M6M) witch is made with the old version 1.xx of the configuration software 
	could not be read with the new Software.
	Error solved (MM)


MMS 6125:
	By the modules MMS 6125 und 6140 was an error in the FFT calculation of the time function screen.
	Error solved (MM)

MMS 3910:
	Stored confirurations witch have been integrated an MMS 3311 module could not be read in again.
	Error solved (MM)
	
	A compare function is added. It is possible to compare the PC configuration with a connected module 
	or with a stored file (*iMC3). 

MMS 3220:
	The print out of the module prints out all pages of all subtypes. (Shaft deflection, Min Max, Eccentricity). 
	Error solved (MM)




== Created on the 16.09.2008 Emerson CSI Version 2.06 Release 02 ==

Changes in the Emerson CSI Version 2.06 Release 02 from 16.09.2008

Generally:
	In the print of a configuration is give out a wronge version number.
 	Error solved
	
	In the command "Send all configuration" comes up an error, that not all modules 
	could set with the right subtype.
 	Error solved

MMS 6910:
	By the connection with a CSI 6824, were it possible that the software show more than one window for the module. 
 	Error solved

MMS 6855:
	For the modules 6140, 6125, 6210, 6220, 6410 and 6418 were the OPC tag "Speed" allways set with 0.
 	Error solved

MMS 6120:
	In the configuration software of the site "Channel" in the 6120 module, 
	the sofware is not calculating new the permissible range of the "measurement range" 
	when the "Integration frequency" is changed.
	So the measurement range is control with wronge values and it is possible,
	that wronge values were send to the module. The module control the values again 
	and deside to deactivate the channel. Error solved

MMS 6824:
	The firmware and the configuration software are modified for config a new "Standard gateway TCPIP Number"
	in the module. This is nessesarry for use two different subnets. 




== Created on the 24.07.2008 Emerson CSI Version 2.06 Release 01 ==

Changes in the Emerson CSI Version 2.06 Release 01 from 24.07.2008

Generally:
	The translation "Englisch" in the Menu Language is now ok.

	In the window "Timefunction" was an error with the translation of the axis channel 1 and channel 2.
	If the Module was not connected the program show allways the German text. 
	Up to now, the name is only shown when the module is connected.

	In the connection with the secundäry master MMS 6824, was an error by the command "Bus Scan".
 	Error solved

	The new Online Help for the CSI Version is implemented.

	Up to now a new version of the VxComm driver for the connection MMS 6825 is deliever.

MMS 6910:
	It is possible to add the Service Data of an module to the print out of the configuration.
	This function can be activate with an ini entry. The data has to be collected with an open dialog Service

MMS 6855:
	The Application use 99% of the CPU if there are more than 20 connctions.
	Now the Program work with less CPU preformance.

MMS 6125:
	The Module MMS 6125/10 is released for the MMS 6910 version.

MMS 6824:
	The module MMS 6211 is deleted from the drag and drop list of the MMS 6824 Gateway module.

	The old subtypes (6220 two channel CGAP and 6220 two channel PP GAP) are deleted. They are not longer in use.

	The subtype „Absolute shaft position“ is added for the MMS 6210.

MMS 6825:
	The module is now deliever with the new firmware version 3.2.2.3.

MMS 3311:
	The module MMS 3311 is released.


